; This is a Setup information file for monitors  with ICM  file; 
; Copyright 2012 Acer International Electronic AG 


[version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%Packbell%
CatalogFile=Maestro226DX.cat
DriverVer=04/10/2013,1.0.0.0


[ControlFlags]
ExcludeFromSelect.NT=Monitor\PKB036D

[DestinationDirs]
DefaultDestDir  = 11
Maestro226DX.copyfiles = 23

[SourceDisksNames]
1=%diskname%,,,

[SourceDisksFiles]
Maestro226DX.icm=1

;Monitor class function driver loading parameters
[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys


[Manufacturer]
%Packbell%=Packbell,NTx86,NTAMD64

[Packbell]
%Maestro226DX%=Maestro226DX.Install, Monitor\PKB036D

[Packbell.NTx86]
%Maestro226DX%=Maestro226DX.Install, Monitor\PKB036D

[Packbell.NTAMD64]
%Maestro226DX%=Maestro226DX.Install, Monitor\PKB036D


[Maestro226DX.Install]
PKBReg=PKB_CURRENT_REG
AddReg=Maestro226DX.AddReg
CopyFiles=Maestro226DX.CopyFiles

[Maestro226DX.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[PKB_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile


[Maestro226DX.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-80.0,50.0-76.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"Maestro226DX.icm"

[Maestro226DX.CopyFiles]
Maestro226DX.ICM


[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

Packbell="Packbell Incorporated"
diskname="Packbell Monitor Maestro226DX Installation Disk"

Maestro226DX="Maestro226DX"

