; nas242w.inf
; Setup information file for NEC AS242W Monitor
;
; Copyright 2015, NEC Display Solutions, Ltd.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NECDS%
CatalogFile=nas242w.cat
DriverVer=09/04/2015,1.15.0904.1728

[ControlFlags]
ExcludeFromSelect.nt=Monitor\NEC2B68
ExcludeFromSelect.nt=Monitor\NEC2B69

[DestinationDirs]
AS242W.CopyFiles = 23
DefaultDestDir = 11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
nas242w.icm=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Manufacturer]
%NECDS%=NECDS,ntamd64

[NECDS]
%AS242W-A%=AS242W-A.Install, Monitor\NEC2B68
%AS242W-D%=AS242W-D.Install, Monitor\NEC2B69

[NECDS.ntamd64]
%AS242W-A%=AS242W-A.Install.ntamd64, Monitor\NEC2B68
%AS242W-D%=AS242W-D.Install.ntamd64, Monitor\NEC2B69

[AS242W-A.Install]
DelReg=DEL_CURRENT_REG
AddReg=AS242W-A.AddReg, 1920, DPMS
CopyFiles=AS242W.CopyFiles

[AS242W-D.Install]
DelReg=DEL_CURRENT_REG
AddReg=AS242W-D.AddReg, 1920, DPMS
CopyFiles=AS242W.CopyFiles

[AS242W-A.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=AS242W-A.AddReg, 1920, DPMS
CopyFiles=AS242W.CopyFiles

[AS242W-D.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=AS242W-D.AddReg, 1920, DPMS
CopyFiles=AS242W.CopyFiles

[AS242W.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install; install monitor class function driver

[AS242W.Install.ntamd64.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install; install monitor class function driver

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1920]
HKR,,MaxResolution,,"1920,1080"

[DPMS]
HKR,,DPMS,,1

[AS242W-A.AddReg]
HKR,"MODES\1920,1080",Mode1,,"31.0-83.0,55.0-76.0,+,+"
HKR,,ICMProfile,0,"nas242w.icm"

[AS242W-D.AddReg]
HKR,"MODES\1920,1080",Mode1,,"31.0-83.0,55.0-76.0,+,+"
HKR,,ICMProfile,0,"nas242w.icm"

[AS242W.CopyFiles]
nas242w.icm

[Strings]
NECDS="NEC"
AS242W-A="NEC AS242W(Analog)"
AS242W-D="NEC AS242W(Digital)"
Disk1="NEC Display Solutions Installation Disk"

SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

AS242W="NEC AS242W"
