;//////////////////////////////////////////////////
;VP5083 dirver-------------IR inf
///////////////////////////////////////////////////
[Version]
signature="$CHICAGO$"

Class=HIDClass
ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}

Provider="Twinhan"
DriverVer=07/25/2005,0.0.1.1


[Manufacturer]
"Twinhan"=Twinhan

[SourceDisksNames]
1="Twinhan VP5083 Drivers",,,""

[SourceDisksFiles]
TV5083IR.sys=1

[Twinhan]

;motorola
%VP5083.DeviceDesc%=VP5083_IR,         PCI\VEN_14F1&DEV_8804&SUBSYS_00201822


[VP5083_IR]
Include=    ks.inf
Needs=      KS.Registration
AddReg=     CX88IR.AddReg,VP5083_IR.AddReg
CopyFiles=  CX88IR.CopyDrivers


[DestinationDirs]
CX88IR.CopyDrivers=10,system32\drivers

[CX88IR.CopyDrivers]
TV5083IR.sys

[CX88IR.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,TV5083IR.sys

;
; Driver Configuration Registry Entries
;

[VP5083_IR.AddReg]
;NEC standard
HKR,"DriverData","IR_Standard",0x00010001, 0x01, 0x00, 0x00, 0x00
;command table 2: small gray remote
HKR,"DriverData","IR_Command_Table",0x00010001, 0x02, 0x00, 0x00, 0x00
;
; Services installation
;

[VP5083_IR.Services]
AddService = CX88IR,2,VP5083.ServiceInstall


[VP5083.ServiceInstall]
DisplayName   = %VP5083.DeviceDesc%
ServiceType   = 1
StartType     = 2
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\TV5083IR.sys
;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]

VP5083.DeviceDesc         = "VP5083 IR Decoder"


