

VeriMark Desktop Fingerprint Key Driver Installation SOP

1. **Download** Verimark Desktop driver from the support site
2. **Connect** **VeriMark Desktop** Security Key to your computer.
3. Go to **Device Manager** and identify the connected VeriMark device under Other devices.
4. **Find** VeriMark Desktop under **“Other devices”** or under **“Biometric devices”** (VeriMark DT Fingerprint Key should be displayed with an exclamation mark indicating the driver needs to be updated) and right click on it and click on **Update Driver.**


**Other devices**




**Biometric devices**




1. **Choose** ‘’Browse My Computer for drivers’’.



1. Indicate the path to the folder where the driver is stored.



1. **Install** driver successfully then click close



1. You are all set and please **restart** before use