;
; Installation file (.inf) for the Capture device.
;
; (c) Copyright 2002 GeoVision Inc.
;

[Version]
LayoutFile=Layout.inf, Layout1.inf, Layout2.inf
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%Msft%

[ControlFlags]
;ExcludeFromSelect=*

[Manufacturer]
%MsftMfg%=Manufact

[Manufact]
%DVR.AudioDeviceDesc%=AudioSection,PCI\VEN_109E&DEV_0878

;--------------
; Audio Section
;--------------

[AudioSection]
AddReg=     ADVR.AddReg
CopyFiles=  ADVR.CopyDrivers
KnownFiles= ADVR.KnownFiles

[ADVR.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,AGV250.sys

[ADVR.CopyDrivers]
AGV250.sys

[ADVR.KnownFiles]
AGV250.sys=safe

[DestinationDirs]
ADVR.CopyDrivers=10,system32\drivers

[AudioSection.Services]
AddService = AGV250,0x00000002,AudioSection.ServiceInstall

[AudioSection.ServiceInstall]
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\system32\drivers\AGV250.sys

[Strings]
Msft=			"GeoVision Inc."
MsftMfg=		"GeoVision Inc."
DVR.AudioDeviceDesc=	"GV250 Audio"

SERVICE_KERNEL_DRIVER=1
SERVICE_DEMAND_START=3
SERVICE_ERROR_NORMAL=1
